//ControlPoints.mat

File that defines set of control points. Each row is a single control point.
Structure is as follows:
[r_coordinate phi_coordinate z_coordinate temperature]

As of now, every element should have ONLY 1 control point, which is NOT in the overlaying parts. Thats the reason, why SetElements outputs number of elements into console.

//Interp.csv

File containing data about conductivity and temperature-enthalpy relationship.


//TechSettings.txt

Technival specifications of the problem
R
L
T_inf (C)
T_in (C)
v_z0 (m/min)
htc (cooling)
v_z1 (m/min)

//NumSettings.txt
Numerical model's settings:
dr0
dz0
dphi (coefficient c in c*pi,c<1)
dtau
pmax


